
SnP Filename convention:

S_PExxxx_Temperature_VDD_AttenuationSetting_Serial#_Insertion

Example file:

S_PE43705_25C_3.400V_22.50dB_SN1_A.s2p

S = Scalar de-embedding of PCB trace S-Parameters has been applied to the data
    (if S is not pre-pended to the filename, the data is not de-embedded)

PExxxx = Product number
Temperature = Temperature of DUT when measured
VDD = VDD of test iteration
AttenuationSetting = Attenuation Setting of part tested
Serial# = serial number of part tested
Insertion = Is rarely used and will show as A. this will change if multiple
            insertions are required to collect all S-parameters of a device with
            more than 12 RF ports.
____________________________________
VNA port defintions:
Port 1 = Pin/J4
Port 2 = Pout/J5
____________________________________
PCB Part Number = 101-0312-05
PCB Date Code = 2311
____________________________________
De-embedding Date = 05/24/2013
Engineer = SKH